 
Date: 12/04/02
 
Plexus Fab PO Number: 
Plexus Job Number: 581005e0	
Customer: Sigmet
Customer Part Name: IO-62 Revision: B

*** File Parameters List ***
 
Layers file format:     Gerber274x
     Number format:     2.5
     Zero suppression:  none
     Number units:      inch
     Coordinate system: absolute
 
     IO-62_B.psl   Gerber Primary Side Silkscreen
     IO-62_B.ppa   Gerber Primary Side Solder Paste
     IO-62_B.pmk   Gerber Primary Side Soldermask
     IO-62_B.l01   Gerber Layer 01
     IO-62_B.l02   Gerber Layer 02
     IO-62_B.l03   Gerber Layer 03
     IO-62_B.l04   Gerber Layer 04
     IO-62_B.l05   Gerber Layer 05
     IO-62_B.l06   Gerber Layer 06
     IO-62_B.l07   Gerber Layer 07
     IO-62_B.l08   Gerber Layer 08
     IO-62_B.smk   Gerber Secondary Side Soldermask
     IO-62_B.spa   Gerber Secondary Side Solder Paste
     IO-62_B.ssl   Gerber Secondary Side Silkscreen
     IO-62_B.vcp   Gerber Via Cap Primary Side

     IO-62_B_fab.art      Gerber Fabrication Drawing
     IO-62_B_fab.hpgl     HPGL Fabrication Drawing
     IO-62_B_fab.dxf      DXF fabrication Drawing
     IO-62_B_fab.pdf      PDF fabrication Drawing
     IO-62_B_tassy.art    Gerber Primary Assembly Drawing
     IO-62_B_tassy.hpgl   HPGL Primary Assembly Drawing
     IO-62_B_tassy.dxf    DXF Primary Assembly Drawing
     IO-62_B_tassy.pdf    PDF Primary Assembly Drawing
     IO-62_B_bassy.art    Gerber Secondary Assembly Drawing
     IO-62_B_bassy.hpgl   HPGL Secondary Assembly Drawing
     IO-62_B_bassy.dxf    DXF Secondary Assembly Drawing
     IO-62_B_bassy.pdf    PDF Secondary Assembly Drawing
     
     IO-62_B.brd   Allegro Data base file
     IO-62_B.odb   Valor ODB++ Database 
    
     IO-62_B.ckt   Genrad Test File
     IO-62_B.val   Fabmaster file
     IO-62_B.uni   Unicam file
     IO-62_B.b     Extraction for  Brd \
     IO-62_B.p     Extraction for  Pad - CIMBRIDGE
     IO-62_B.s     Extraction for  Sym -   FILES
     IO-62_B.r     Extraction for  Rte /  
     smd_top.rpt    Surface mount comps topside with fid's
     smd_bot.rpt    Surface mount comps botside with fid's
     thru_hole.rpt  Thru-hole comps
     placed.rpt     Placement file, X-Y coordinates
     sympin.rpt     Symbol pins report
     netlist.rpt    Netlist report
     IO-62_B.ipc   IPC356D file
     IO-62_B.drl   Ncdrill file
     IO-62_B.dpm   Ncdrill parmeter file
     art_aper.txt   Gerber Aperture list
     art_param.txt  Gerber Parameter File 

---->For questions call number below and reference Plexus# 581005e0
Primary Contact: Roland Cossette  Position: Design Support 
   1st #: 603-864-1306  Times Avail: days
   2nd #: 603-424-4281  Times Avail: nights
Secondary Contact: Joe Page  Position: Design Services Manager
   1st #: 603-864-1315  Times Avail: days
Alternate Contact: Michael DeStefano  Position: Design Support
   1st #: 603-863-1326  Times Avail: days
   
