 
Date: 10/16/02
 
Plexus Fab PO Number: 
Plexus Job Number: 581003e0	
Customer: Sigmet
Customer Part Name: RVP8-RX Revision: B

*** File Parameters List ***
 
Layers file format:     Gerber274x
     Number format:     2.5
     Zero suppression:  none
     Number units:      inch
     Coordinate system: absolute
 
     RVP8-RX_B.psl   Gerber Primary Side Silkscreen
     RVP8-RX_B.ppa   Gerber Primary Side Solder Paste
     RVP8-RX_B.pmk   Gerber Primary Side Soldermask
     RVP8-RX_B.l01   Gerber Layer 01
     RVP8-RX_B.l02   Gerber Layer 02
     RVP8-RX_B.l03   Gerber Layer 03
     RVP8-RX_B.l04   Gerber Layer 04
     RVP8-RX_B.l05   Gerber Layer 05
     RVP8-RX_B.l06   Gerber Layer 06
     RVP8-RX_B.l07   Gerber Layer 07
     RVP8-RX_B.l08   Gerber Layer 08
     RVP8-RX_B.smk   Gerber Secondary Side Soldermask
     RVP8-RX_B.spa   Gerber Secondary Side Solder Paste
     RVP8-RX_B.ssl   Gerber Secondary Side Silkscreen

     RVP8-RX_B_fab.art      Gerber Fabrication Drawing
     RVP8-RX_B_fab.hpgl     HPGL Fabrication Drawing
     RVP8-RX_B_fab.dxf      DXF fabrication Drawing
     RVP8-RX_B_fab.pdf      PDF fabrication Drawing
     RVP8-RX_B_tassy.art    Gerber Primary Assembly Drawing
     RVP8-RX_B_tassy.hpgl   HPGL Primary Assembly Drawing
     RVP8-RX_B_tassy.dxf    DXF Primary Assembly Drawing
     RVP8-RX_B_tassy.pdf    PDF Primary Assembly Drawing
     RVP8-RX_B_bassy.art    Gerber Secondary Assembly Drawing
     RVP8-RX_B_bassy.hpgl   HPGL Secondary Assembly Drawing
     RVP8-RX_B_bassy.dxf    DXF Secondary Assembly Drawing
     RVP8-RX_B_bassy.pdf    PDF Secondary Assembly Drawing
     
     RVP8-RX_B.brd   Allegro Data base file
     RVP8-RX_B.odb   Valor ODB++ Database 
    
     RVP8-RX_B.ckt   Genrad Test File
     RVP8-RX_B.val   Fabmaster file
     RVP8-RX_B.uni   Unicam file
     RVP8-RX_B.b     Extraction for  Brd \
     RVP8-RX_B.p     Extraction for  Pad - CIMBRIDGE
     RVP8-RX_B.s     Extraction for  Sym -   FILES
     RVP8-RX_B.r     Extraction for  Rte /  
     smd_top.rpt    Surface mount comps topside with fid's
     smd_bot.rpt    Surface mount comps botside with fid's
     thru_hole.rpt  Thru-hole comps
     placed.rpt     Placement file, X-Y coordinates
     sympin.rpt     Symbol pins report
     netlist.rpt    Netlist report
     RVP8-RX_B.ipc   IPC356D file
     RVP8-RX_B.drl   Ncdrill file
     RVP8-RX_B.dpm   Ncdrill parmeter file
     art_aper.txt   Gerber Aperture list
     art_param.txt  Gerber Parameter File 

---->For questions call number below and reference Plexus# 581003e0
Primary Contact: Roland Cossette  Position: Design Support 
   1st #: 603-864-1306  Times Avail: days
   2nd #: 603-424-4281  Times Avail: nights
   Pager: 603-561-2710 24 hours
Secondary Contact: Joe Page  Position: Design Services Manager
   1st #: 603-864-1315  Times Avail: days
   Alternate Contact: Michael DeStefano  Position: Design Support
   1st #: 603-864-1326  Times Avail: days
   
