 
Date: 03/17/04
 
 Fab PO Number: 
Freedom CAD Job Number: 581002f0	
Customer: Sigmet
Customer Part Name: RVP8-RX Revision: C

*** File Parameters List ***
 
Layers file format:     Gerber274x
     Number format:     2.4
     Zero suppression:  none
     Number units:      inch
     Coordinate system: absolute
 
     RVP8-RX_C.psl   Gerber Primary Side Silkscreen
     RVP8-RX_C.ppa   Gerber Primary Side Solder Paste
     RVP8-RX_C.pmk   Gerber Primary Side Soldermask
     RVP8-RX_C.l01   Gerber Layer 01
     RVP8-RX_C.l02   Gerber Layer 02
     RVP8-RX_C.l03   Gerber Layer 03
     RVP8-RX_C.l04   Gerber Layer 04
     RVP8-RX_C.l05   Gerber Layer 05
     RVP8-RX_C.l06   Gerber Layer 06
     RVP8-RX_C.l07   Gerber Layer 07
     RVP8-RX_C.l08   Gerber Layer 08
     RVP8-RX_C.smk   Gerber Secondary Side Soldermask
     RVP8-RX_C.spa   Gerber Secondary Side Solder Paste
     RVP8-RX_C.ssl   Gerber Secondary Side Silkscreen
     RVP8-RX_C.vcp   Gerber Primary Side Via Cap

     RVP8-RX_C_fab.art      Gerber Fabrication Drawing
     RVP8-RX_C_fab.hpgl     HPGL Fabrication Drawing
     RVP8-RX_C_fab.dxf      DXF fabrication Drawing
     RVP8-RX_C_fab.pdf      PDF fabrication Drawing
     RVP8-RX_C_tassy.art    Gerber Primary Assembly Drawing
     RVP8-RX_C_tassy.hpgl   HPGL Primary Assembly Drawing
     RVP8-RX_C_tassy.dxf    DXF Primary Assembly Drawing
     RVP8-RX_C_tassy.pdf    PDF Primary Assembly Drawing
     RVP8-RX_C_bassy.art    Gerber Secondary Assembly Drawing
     RVP8-RX_C_bassy.hpgl   HPGL Secondary Assembly Drawing
     RVP8-RX_C_bassy.dxf    DXF Secondary Assembly Drawing
     RVP8-RX_C_bassy.pdf    PDF Secondary Assembly Drawing
     
     RVP8-RX_C.brd          Allegro Data base file
     RVP8-RX_C_odb.zip      Valor ODB++ Database 
    
     RVP8-RX_C.ckt          Genrad Test File
     RVP8-RX_C.val          Fabmaster file
     RVP8-RX_C.uni          Unicam file
     RVP8-RX_C.b            Extraction for  Brd \
     RVP8-RX_C.p            Extraction for  Pad - CIMBRIDGE
     RVP8-RX_C.s            Extraction for  Sym -   FILES
     RVP8-RX_C.r            Extraction for  Rte /  
     smd_top.rpt            Surface mount comps topside with fid's
     smd_bot.rpt            Surface mount comps botside with fid's
     thru_hole.rpt          Thru-hole comps
     placed.rpt             Placement file, X-Y coordinates
     sympin.rpt             Symbol pins report
     netlist.rpt            Netlist report
     RVP8-RX_C.ipc          IPC356D file
     RVP8-RX_C.drl          Ncdrill file
     RVP8-RX_C.dpm          Ncdrill parmeter file
     art_aper.txt           Gerber Aperture list
     art_param.txt          Gerber Parameter File 

---->For questions call number below and reference FCS# 581002f0
Primary Contact: Roland Cossette  Position: Design Support 
   1st #: 603-864-1306  Times Avail: days
   2nd #: 603-424-4281  Times Avail: nights
   Secondary Contact: Lauren Primmer  Position: Operations Manager
   1st #: 603-864-1300 x1348  Times Avail: days
   2nd #: 603-672-2725  Times Avail: nights
   
 
